For 1990-2009 cars

Checks | Causes
--- | ---
2-6 Clutch Assembly |

• | Inspect for worn or improper surface finish on the 2-6 Clutch Plates (446, 447) and Backing Plate (448)

• | Inspect for fatigued 2-6 Clutch Piston Cushion Spring (445)

Case Cover Assembly (403) |

• | Inspect for damaged or broken 2-6 Clutch Piston (405) and piston seals damaged, worn or delaminating

• | Inspect for fatigued 2-6 Clutch Piston Return Spring (406)