For 1990-2009 cars

## Rear Seat Back Filler Panel Replacement with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Outer Finish Cover

#### Procedure

1. Release the seat to the full forward position.
2. Remove the rear seat recliner outer finish cover by pulling outward to disengage the retainers.

2 | Rear Seat Recliner Outer Finish Cover

#### Procedure

Remove the rear seat recliner outer finish cover by pulling outward to disengage the retainers.

3 | Rear Seat Back Cushion Filler Panel Push-in Retainer (Qty: 2)
4 | Rear Seat Back Cushion Filler Panel

#### Procedure

Pull rearward to disengage the retainers.