For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat No. 2 back cushion cover and pad. Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement.

1 | Rear Seat No. 2 Head Restraint Bracket Cover Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat No. 2 Head Restraint Bracket Cover
3 | Rear Seat No. 2 Head Restraint Bracket Bolt (Qty: 3) Tighten 15 N·m (11 lb ft)
4 | Rear Seat No. 2 Head Restraint Bracket

#### Procedure

Disconnect the cables from the head restraint bracket.