For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the outside door handle. Refer to Front Side Door Outside Handle Replacement .
4. Remove the front side door outside handle housing. Refer to Front Side Door Outside Handle Housing Replacement .

1 | Lock Cylinder Clip Tip Use a flat-bladed tool to remove the clip.
2 | Front Door Lock Cylinder Tip Pull the lock cylinder from the housing to remove.