For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

It is only necessary to lower the headliner. Only do those step in headliner replacement that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement .

1 | Sunroof Drain Hose Retainers (Qty: 8)
2 | Sunroof Drain Hose

#### Procedure

1. Disconnect the sunroof drain hose from the sunroof module spigot.
2. When install drain hoses, ensure to route the end of the drain hose through the access hole in the side quarter panel to prevent interior water leaks.