For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Hinge Upper Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Upper Hinge Tip Check the door for proper alignment, then adjust as necessary.
4 | Rear Side Door Hinge Lower Bolt Tip After installation of the replacement upper hinge, from the underside of the hinge, remove the temporary keeper pivot bolt and replace with longer permanent bolt. Tighten 25 N·m (18 lb ft)
5 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
7 | Rear Side Door Lower Hinge Tip Check the door for proper alignment, then adjust as necessary.