For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Liftgate Strut Warning: When a lift gate hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury. Caution: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

#### Procedure

• | Release the locking tabs on the strut.

• | Ensure the clip is fully seated when rod is reinstalled. If the clip cannot be fully seated, a new rod should be installed.