For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the driver side front carpet retainer. Refer to Front Side Door Opening Floor Carpet Retainer Replacement.
3. Disconnect the park brake warning indicator switch electrical connector.

1 | Park Brake Warning Lamp Switch Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Park Brake Warning Lamp Switch