For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Front Lower Control Arm Bushing Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 195 N·m (144 lb ft)
2 | Front Lower Control Arm Bushing Bolt (Qty: 2) Note: When tightening the bolt to specifications, hold the bolt and torque the nut for the proper torque.
3 | Lower Control Arm Front Bushing Nut (Qty: 2) Tighten 75 N·m (55 lb ft)
4 | Front Lower Control Arm Bushing Note: The control arm bushing is NOT serviced separately, but with the mounting bracket