For 1990-2009 cars

## Front Door Frame Applique Replacement OUTLOOK/Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Place the front door window in the full down position.
2. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement.
3. Remove the front door window inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement.

1 | Front Door Applique Rivet (Qty: 2)

#### Procedure

1. Apply masking tape to the door frame and applique.
2. Pull the window channel weatherstrip from the applique to expose the rivets.
3. Drill out the rivets to remove the applique.

2 | Front Door Applique Tip Pull the applique up and out of the door.

## Front Door Frame Applique Replacement Enclave

### Stripes or Decals

The stripes and decals adhere to a painted surface using pressure sensitive adhesive.

The use of a wetting solution aids the technician in lifting and positioning the stripe or decal during the installation. The wetting solution ensures a better bond between the stripe or decal and the panel assembly. Use a wetting solution when applying large stripe and decal packages.

Complete the following procedures before you apply a stripe or a decal:

1. Place the front door window in the full down position.
2. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
3. Remove the front door window inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .

• | Metal repair or refinishing after a collision

• | Painting the underlying surface

Maintain a temperature 21-38°C (70-100°F) on the body surfaces and the decals prior to installation. The decal requires auxiliary heat sources in order to warm the body surfaces and decals. If the temperature is below 21°C (70°F) the decal may not adhere to the body surface properly.

Important: You may apply stripes or decals using the dry method. Use the wet method if the dry method does not result in a bubble free application. This may be the case in large graphics packages.

Use the wet method in order to apply the stripes or decals that are applied on flexible surfaces (fascias, etc.). This will reduce the formation of bubbles under the decal due to the outgassing potential of the flexible materials.

Use the following equipment and materials in order to apply a stripe or a decal:

• | A wetting solution

| A foaming type of window cleaner that does not contain ammonia.

• | A silicone, wax and grease remover

• | Varnish Makers and Painters (VM&P) Naptha

• | Isopropyl alcohol

• | A squeegee

- | 75-100 mm (3-4 in) wide

- | Made of plastic or hard rubber

- | Deburr any sharp or rough edges in order to prevent scratching of the stripe or decal.

• | A water bucket and sponge or spray bottle

• | Sandpaper

- | 800 grit or finer

- | Wet or dry type

• | A heat gun J 25070

• | A clean, lint-free wiping cloth

• | A sharp knife or razor blade

• | A pair of scissors

• | A fine pin or needle

• | A marking pencil

### Stripe or Decal Removal

1. Remove the following components:

• | Necessary moldings or trim panel

• | Molding attaching clips

• | Handles

• | Sidemarker lamps

• | Other stripe or decal overlapping parts

2. Clean the following areas as needed:

• | The repair surfaces

• | The adjacent panels

• | The openings

3. Use 3M™ ScotchBrite molding adhesive remover disk 3M™ P/N 07502 or equivalent in order to remove the stripe or decal from the body panel.
4. Use Varnish Makers and Painters (VM&P) Naptha to remove all traces of adhesive residue from the painted surfaces.

### Stripe or Decal Installation -- Wet Method

1. Place the front door window in the full down position.
2. Remove the front door window inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
3. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
4. Prepare the surface.

Important: Remove any imperfections that would appear through the stripe or decal if the area has been refinished.

5. Clean the painted surface using the following types of removers:

• | Silicone

• | Wax

• | Grease

6. Clean the area where the stripe or decal will be applied using a 50-50 mixture of isopropyl alcohol and water.
7. Wipe the panel surface using a clean cloth while the solvent is still wet. Allow the panel surface to dry.
8. Apply the wetting solution to the area where you are installing the stripe or decal.

Application of a soapy wetting solution on the top side of the stripe or decal will ease the pull of the squeegee on the stripe or decal.

Important: Do not touch the adhesive backing of the stripes.

9. Apply the wetting solution on the adhesive side of the stripe or decal.

Remove the backing material of the stripe or the decal as needed.

10. Apply the strip or decal to the panel. The wetting solution will allow movement for proper positioning on the panel surface.
11. Working from the center where possible, squeegee the stripe or decal into position. Apply additional wetting solution as needed to ease installation.
12. Apply heat to the stripe or decal at the recessed areas. Press the stripe or decal into the recess to obtain a firm bond.
13. Use adequate light reflection to inspect the stripe or decal from a critical angle. This technique detects any irregularities that may have developed during the installation.

Important: Do not use a razor blade or a knife edge to pierce the air bubbles.

14. Remove all air bubbles by piercing the bubble with one of the following items:

• | A safety pin

• | A needle

• | A tool with the same size piercing tip

15. Pierce the bubble on the outer edge. Force the air out through the opposite edge using the blade of the squeegee.
16. Install any previously removed components. Clean the components as needed.