For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .

1 | Rear Seat Back Cushion Panel

#### Procedure

1. Note the routing for installation, the inboard cable should be routed over the outboard cable.
2. Cut off the rosebud retainer to remove and always install a new retainer for installation.
3. Disconnect the seat latch cable.