For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR. Refer to SIR Disabling and Enabling.
2. On back side of the steering wheel are 2 openings, place the wheel so that one opening is on top.
3. Using a blunt-ended tool, push the spring fastener inward through the access hole. Repeat the step for the other opening.

1 | Steering Wheel Inflatable Restraint Module Assembly Tip

1. Release the connector position assurance (CPA) retainer.
2. Disconnect the electrical connectors.
3. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.