For 1990-2009 cars

## Rear Window Wiper Motor Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Remove the rear wiper arm assembly. Refer to Rear Window Wiper Arm Replacement.
3. Disconnect the electrical connector to the rear window wiper motor.

1 | Rear Window Wiper Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Window Wiper Motor Assembly Tip

• | Ensure the rear window wiper pivot shaft seal in the liftgate rear window is not damaged when the wiper motor pivot shaft is pulled from the seal.

• | Replace the pivot shaft seal if damaged.

## Rear Window Wiper Motor Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Remove the rear wiper arm assembly. Refer to Rear Window Wiper Arm Replacement.
3. Disconnect the electrical connector.

1 | Rear Window Wiper Pivot Shaft Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 19 N·m (14 lb ft)
2 | Rear Window Wiper Pivot Shaft Gasket

#### Procedure

Align the tab on the gasket to the slot on the rear wiper motor upon assembly.

3 | Rear Window Wiper Motor Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
4 | Rear Window Wiper Motor Assembly

## Rear Window Wiper Motor Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Remove the rear wiper arm assembly. Refer to Rear Window Wiper Arm Replacement.
3. Disconnect the electrical connector to the rear window wiper motor.

1 | Rear Window Wiper Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Window Wiper Motor Assembly Tip

• | Ensure the rear window wiper pivot shaft seal in the liftgate rear window is not damaged when the wiper motor pivot shaft is pulled from the seal.

• | Replace the pivot shaft seal if damaged.

## Rear Window Wiper Motor Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear liftgate interior trim panel. Refer to Liftgate Trim Panel Replacement.
2. Remove the rear wiper arm assembly. Refer to Rear Window Wiper Arm Replacement.
3. Disconnect the electrical connector.

1 | Rear Window Wiper Arm Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 19 N·m (14 lb ft)
2 | Rear Window Wiper Pivot Shaft Gasket

#### Procedure

Align the tab on the gasket to the slot on the rear wiper motor upon assembly.

3 | Rear Window Wiper Motor Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
4 | Rear Window Wiper Motor Assembly