For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console assembly. Refer to Front Floor Console Replacement.

1 | Radio Front Floor Console Speaker Screws (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Radio Front Floor Console Speaker Assembly

#### Procedure

Disconnect the electrical connector.