For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the coolant. Refer to Cooling System Draining and Filling
2. Remove the front compartment sight shield. Refer to Front Compartment Sight Shields Replacement

1 | Radiator Outlet Hose Clamp (Qty: 2)

#### Procedure

Using J 38185 reposition the radiator outlet hose clamps.

#### Special Tools

J 38185 Hose Clamp Pliers

2 | Radiator Outlet Hose