For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering wheel. Refer to Steering Wheel Replacement.
2. Remove the steering column upper trim cover. Refer to Steering Column Upper Trim Cover Replacement.
3. Remove the steering column lower trim cover. Refer to Steering Column Lower Trim Cover Replacement.
4. Remove the ignition lock cylinder opening trim cover. Refer to Ignition Lock Cylinder Opening Trim Cover Replacement.

1 | Inflatable Restraint Steering Wheel Module Coil Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in).
2 | Inflatable Restraint Steering Wheel Module Coil