For 1990-2009 cars

## Front Fender Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the rocker panel molding. Refer to Rocker Panel Front Molding Replacement.

1 | Front Fender Bolt (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (25 lb in)
2 | Front Fender

## Front Fender Replacement Acadia, Enclave, and OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
3. Remove the rocker panel molding. Refer to Rocker Panel Front Molding Replacement.

1 | Front Fender Bolt (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (25 lb in)
2 | Front Fender Bolt Tip Open the door to access the bolt.
3 | Front Fender