For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the power steering pump. Refer to Power Steering Pump Replacement.

1 | Power Steering Pump Pulley

#### Procedure

1. Use the J 25034-C remover for Buick, GMC, and Chevrolet or the SA9162C remover/installer for Saturn to remove the power steering pump pulley.
2. Use the J 25033-C installer for Buick, GMC, and Chevrolet or the SA9162C remover/installer for Saturn to install the power steering pump pulley.
3. Ensure the axial tolerance of the power steering pulley on the shaft is within 0.25 mm (0.010 in).

#### Special Tools

• | J 25033-C Pulley Installer

• | J 25034-C Pulley Remover

• | SA9162C Power Steering Pump Pulley Remover/Installer

For equivalent regional tools, refer to Special Tools.