For 1990-2009 cars

## Coat Hook Replacement Enclave or Traverse

Callout | Component Name
--- | ---
1 | Coat Hook Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Coat Hook Assembly

#### Procedure

Flip the integral hook downward to access the fastener.

## Coat Hook Replacement Acadia or OUTLOOK

Callout | Component Name
--- | ---
1 | Coat Hook Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Coat Hook Assembly Tip Flip the cover downward to access the fastener.