For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the front floor console. Refer to the appropriate procedure:

• | With front floor console speaker, refer to Front Floor Console Replacement.

• | Without front floor console speaker, refer to Front Floor Console Extension Panel Replacement - Right Side.

3. Remove HVAC floor duct.

1 | Inflatable Restraint Vehicle Rollover Sensor Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (88 lb in)
2 | Inflatable Restraint Vehicle Rollover Sensor Assembly

#### Procedure

1. Position carpet in order to access sensor.
2. Disconnect the electrical connectors.