For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Bucket Seat Replacement .
2. Remove the center pillar lower molding. Refer to Center Pillar Lower Garnish Molding Replacement
3. Remove the rear seats. Refer to Rear Seat Replacement .
4. Remove the rear number 2 seats. Refer to Rear Number 2 Seat Replacement .
5. Remove the rear quarter lower trim. Refer to Quarter Lower Rear Trim Panel Replacement .

1 | Rear Floor Panel Carpet Assembly Tip The front and rear compartment carpet must be installed prior to the rear carpet.