For 1990-2009 cars

#### Special Tools

• | J 5590 Bearing and Seal Driver

• | J-25254-A Oil Seal Installer

| For equivalent regional tools, refer to Special Tools.

### Left Camshaft Cover

1. Install the NEW left spark plug shield tube seals using the J 5590 driver (1) and J-25254-A installer (2).
2. Install the NEW left camshaft cover gasket.
3. Install the oil fill cap.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the fuel injector sight shield cover ballstud and tighten to 10 N·m (89 lb in).

Note: The camshaft cover bolt grommet must be installed into the camshaft cover bolt hole before installing the camshaft cover bolt.

5. Install the NEW left camshaft cover bolt grommets.

### Right Camshaft Cover

1. Install the NEW right spark plug shield tube coil seals using the J 5590 driver (1) and J-25254-A installer (2).
2. Install the NEW right camshaft cover gasket.

Note: The camshaft cover bolt grommet must be installed into the camshaft cover bolt hole before installing the camshaft cover bolt.

3. Install the NEW right camshaft cover bolt grommets.