For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering column lower trim cover. Refer to Steering Column Lower Trim Cover Replacement.

1 | Steering Column Tilt Wheel and Telescope Switch

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Release the plastic retaining tabs to release the switch from the turn signal switch bracket.