For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
3. Remove the rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.

1 | Rear Seat Number 2 Shoulder Belt Anchor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Seat Number 2 Shoulder Belt Guide Adjuster Bolt Tighten 45 N·m (33 lb ft)
3 | Rear Seat Number 2 Shoulder Belt Retractor Bolt Tighten 45 N·m (33 lb ft)
4 | Rear Seat Number 2 Shoulder Belt Retractor Assembly