For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.

1 | Steering Wheel Spoke Cover (Qty: 2) Tip Use a flat-bladed plastic tool to disengage the 2 detent tabs and carefully pull cover from the 2 retainers.
2 | Steering Wheel Control Switch Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Steering Wheel Control Switch Assembly (Qty: 2)

#### Procedure

1. Radio control switch assembly is shown. Cruise control switch assembly is similar.
2. Disconnect the electrical connector.