For 1990-2009 cars

## Rear Seat Support Replacement with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement .

1 | Rear Seat Cushion Spring (Qty: 3)
2 | Rear Seat Support Assembly

## Rear Seat Support Replacement with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement .

1 | Rear Seat Cushion Spring (Qty: 6)
2 | Rear Seat Support Assembly (Qty: 2)

## Rear Seat Support Replacement with Armrest

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Support Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat Support