For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Impact Bar Bracket Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Front Bumper Impact Bar

#### Procedure

• | Disconnect the electrical connectors/harnesses as needed.

• | Transfer any parts as needed.

• | Remove right and left side air baffle attached at the impact bar.