For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the roof console assembly. Refer to Roof Console Replacement.
2. Remove the garage door opener. Refer to Garage Door Opener Replacement.

1 | Utility Overhead Console Bracket Screw (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Utility Overhead Console Bracket

#### Procedure

Disconnect the electrical connection.

3 | Sun Roof Sunshade Switch Assembly
4 | Sun Roof Switch Assembly