For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the Fromt Bumper Fasica. Refer to Front Bumper Fascia Replacement .

1 | Desiccant Cartridge Cap
2 | Desiccant Cartridge Snap Ring

#### Procedure

Lightly tap inward on Desiccant Cartridge plug to gain clearance for snap ring removal.

3 | Desiccant Cartridge Plug

#### Procedure

Insert a 5 mm screw into plug and pull outward for removal.

4 | Desiccant Cartridge

#### Procedure

Use of pliers or vice grips may aid in cartridge removal.