For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right rear quarter trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Disconnect the blower motor control module electrical connector.

1 | Blower Motor Resistor Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Blower Motor Control Module