For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side .
2. Remove the outside rear view mirror (ORVM) wire harness from the water deflector.
3. Carefully remove the water deflector from the door by releasing the adhesive backing.

### Installation Procedure

1. Install the ORVM wire harness to the water deflector.
2. Position the water deflector to the door.
3. Press the water deflector to the door. Ensure that the water deflector forms a proper seal around the surface of the door panel.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side .