For 1990-2009 cars

## High Mount Stop Lamp Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the liftgate.
2. Remove the rear spoiler. Refer to Rear Spoiler Replacement.
3. Place the rear spoiler on a clean protected surface in order to remove the Light Emitted Diode (LED) high mounted stop lamp.

1 | High Mount Stop Lamp Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | High Mount Stop Lamp Electrical Connector
3 | High Mount Stop Lamp Assembly

#### Procedure

Remove the high mount (LED) stop lamp from the bottom side of the rear spoiler.

## High Mount Stop Lamp Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the liftgate.
2. Remove the interior liftgate garnish molding. Refer to Liftgate Garnish Molding Replacement.
3. Remove the rear spoiler. Refer to Rear Spoiler Replacement.

1 | High Mounted Stop Lamp Electrical Connector
2 | High Mounted Stop Lamp Screws (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | High Mount Stop Lamp Assembly

#### Procedure

Remove the high mounted stop lamp from the bottom side of the rear spoiler.

## High Mount Stop Lamp Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the liftgate.
2. Remove the interior liftgate garnish molding. Refer to Liftgate Garnish Molding Replacement.
3. Remove the rear spoiler. Refer to Rear Spoiler Replacement.
4. Place the rear spoiler on a clean protected surface in order to remove the bottom mounted stop lamp.

1 | High Mount Stop Lamp Screws (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | High Mount Stop Lamp Assembly

#### Procedure

Remove the high mount stop lamp from the bottom side of the rear spoiler.

## High Mount Stop Lamp Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the liftgate.
2. Remove the interior liftgate garnish molding. Refer to Liftgate Garnish Molding Replacement.
3. Remove the rear spoiler in order to access the high mounted stop lamp. Refer to Rear Spoiler Replacement.

1 | High Mounted Stop Lamp Electrical Connector
2 | High Mounted Stop Lamp Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | High Mount Stop Lamp Assembly

#### Procedure

Remove the high mounted stop lamp from the bottom side of the rear spoiler.