For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedure

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.

1 | Front Side Door Hinge Upper Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip Replace only one hinge at a time. Tighten
25 N·m (18 lb ft)

2 | Front Side Door Hinge Upper Bolt (Qty: 3) Tighten 25 N·m (18 lb ft)
3 | Front Side Door Hinge Lower Bolt Tip After installation of the replacement upper hinge, from the underside of the hinge, remove the temporary keeper pivot bolt and replace with longer permanent bolt. Tighten 25 N·m (18 lb ft)
4 | Front Side Door Hinge Lower Bolt (Qty: 3) Tighten 25 N·m (18 lb ft)
5 | Front Side Door Hinge Lower Bolt (Qty: 4) Tighten 25 N·m (18 lb ft)