For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Bucket Seat Replacement.

1 | Driver Seat Adjuster Memory Module Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Driver Seat Adjuster Memory Module

#### Procedure

1. Disconnect the electrical connector.
2. Reprogram the module after replacement. Refer to Control Module References.