For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Bolt Access Plug Tip Use a plastic flat-bladed tool to remove.
2 | Rear Side Door Outside Handle Cap Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Rear Door Outside Handle Cap
4 | Rear Door Outside Handle Tip Pull the outside handle rearward to release it from the handle housing.
5 | Rear Door Outside Handle Gasket