For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .

1 | Rear Side Door Inner Window Sealing Strip

#### Procedures

1. Start from the front edge of the door, pull upward on the inner window sealing strip to release it from the pinch-weld flange.
2. Install the inner window sealing strip to the front edge of the door, press firmly onto the pinch-weld flange and work it rearward.