For 1990-2009 cars

## Rearview Camera Replacement Acadia, Enclave, OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate applique. Refer to Liftgate Applique Replacement.

1 | Double Ended Stud with Collar (Qty: 2) Tip Remove in order to remove the isolator from the applique.
2 | Liftgate Applique Isolator Tip Carefully release the isolator tab from the liftgate applique.
3 | Rearview Camera

#### Procedure

1. Disengage the electrical harness from above the rear latch clips.
2. Disconnect the camera electrical harness connector from the rear license plate lamp harness electrical connector.
3. Ensure the electrical harness is properly positioned prior to installation of the liftgate applique isolator.

## Rearview Camera Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate outside handle. Refer to Liftgate Outside Handle Replacement.

1 | Rearview Camera Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rearview Camera Tip Release tape to remove the wiring harness.