For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.

1 | Steering Wheel Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Steering Wheel

#### Procedure

1. Disconnect all electrical connectors as needed.
2. Remove the steering wheel using the J 1859-A puller and the J 42578 puller legs .

#### Special Tools

• | J 1859-A Steering Wheel Puller

• | J 42578 Steering Wheel Puller Legs