For 1990-2009 cars

## Rear Seat Cushion Cover and Pad Replacement with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the seat to the Smart Slide® E-Z entry position.
2. Remove the rear seat cushion trim panels. Refer to Rear Seat Cushion Trim Panel Assembly Replacement - Outboard or Rear Seat Cushion Trim Panel Assembly Replacement - Inboard .
3. Remove the rear seat cushion front cover. Refer to Rear Seat Cushion Front Cover Replacement .

1 | Rear Seat Cushion Cover

#### Procedure

1. Disengage the seat cushion cover j-channel from the seat cushion frame.
2. Remove the hog rings that retain the rear of the seat cushion cover to the frame.
3. Disconnect the rear seat latch cables.
4. Remove the rear seat cushion cover and pad as an assembly.

2 | Rear Seat Cushion Pad

#### Procedure

1. Disengage the hog rings retaining the cover to the pad.
2. Separate the seat cushion cover from the pad.

## Rear Seat Cushion Cover and Pad Replacement with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the seat to the Smart Slide® E-Z entry position.
2. Remove the rear seat cushion trim panel assembly. Refer to Rear Seat Cushion Trim Panel Assembly Replacement - Inboard or Rear Seat Cushion Trim Panel Assembly Replacement - Outboard .
3. Remove the rear seat cushion trim panel assembly. Refer to Rear Seat Cushion Trim Panel Replacement - Inner Outboard or Rear Seat Cushion Trim Panel Replacement - Inner Inboard .
4. Remove the rear seat adjuster handle. Refer to Rear Seat Adjuster Handle Replacement .
5. Remove the rear seat cushion front cover. Refer to Rear Seat Cushion Front Cover Replacement .

1 | Rear Seat Cushion Cover

#### Procedure

1. Disengage the seat cushion cover j-channel from the seat cushion frame.
2. Remove the hog rings that retain the rear of the seat cushion cover to the frame.
3. Disconnect the rear seat latch cables.
4. Remove the rear seat cushion cover and pad as an assembly.

2 | Rear Seat Cushion Pad

#### Procedure

1. Disengage the hog rings retaining the cover to the pad.
2. Separate the seat cushion cover from the pad.