For 1990-2009 cars

## Rear Seat Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat track covers. Refer to Rear Seat Track Front Inboard Cover, Front Outboard Cover, Rear Inboard Cover, and Rear Outboard Cover Replacement.

1 | Rear Seat No. 1 Assembly Bolt (Qty: 14) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat Assembly (Qty: 2)

## Rear Seat Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat track covers. Refer to Rear Seat Track Front Inboard Cover, Front Outboard Cover, Rear Inboard Cover, and Rear Outboard Cover Replacement.

1 | Rear Seat No. 1 Assembly Bolt (Qty: 12) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat Assembly (Qty: 2)