For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lift gate interior trim panel. Refer to Liftgate Trim Panel Replacement

1 | Back Up Lamp Applique Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Integral Clip (Qty: 2)
3 | Back Up Lamp Applique Assembly Tip Disconnect the bulb socket from the applique.