For 1990-2009 cars

### Tilt/Telescoping Soft Stops

After replacement of the memory seat module (MSM), it is necessary to program the tilt/telescoping soft stops. Each soft stop is a programmable end of travel that is set approximately 1.3 cm (0.5 in) from the mechanical end of travel. The steering column has a soft stop set at each end of the telescoping in/out and tilt up/down movement. The system uses soft stops to prevent wear on the system by ensuring that the steering column movement stops before it reaches its mechanical end of travel in any direction. The soft stops are initially programmed at the factory. The stop positions may be reprogrammed, which is necessary any time the MSM, the tilt actuator or telescope actuators replaced, as described in the following procedure.

### Tilt/Telescoping Soft Stop Programming Procedure

1. Turn ON the ignition, with the engine OFF.
2. Connect a scan tool to the vehicle.
3. Select Model Year.
4. Select LD Truck.
5. Select Buick.
6. Product Line (R).
7. Select Body.
8. Select Memory Seat
9. Select Special Functions
10. Select Driver Seat.
11. Select Learn Column Soft Stops.
12. Follow the scan tool on-screen instructions.