For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front floor console extension panel - right side. Refer to Front Floor Console Extension Panel Replacement - Right Side .
2. Remove the instrument panel insulator - right side. Refer to Instrument Panel Insulator Panel Replacement - Right Side .

1 | Air Temperature Sensor - Lower Right

#### Procedure

1. Disconnect the electrical connector.
2. Grasp and pull sensor straight outward from HVAC case.