For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the wheel bearing/hub assembly. Refer to Front Wheel Bearing and Hub Replacement.
3. Remove the outer tie rod end from the steering knuckle. Refer to Steering Linkage Outer Tie Rod Replacement.
4. Separate the lower ball joint from the steering knuckle. Refer to Lower Control Arm Ball Joint Replacement.

1 | Front Strut Suspension Nut (Qty: 2)
2 | Front Strut Suspension Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Support the wheel drive shaft with mechanics wire after the knuckle has been removed. Tighten
195 N·m (144 lb ft)

3 | Steering Knuckle