For 1990-2009 cars

Table 1: | Fluid Seal Ring Installation
Table 2: | 2-6 Clutch Piston Installation
Table 3: | Low and Reverse Clutch Piston Installation
Table 4: | 2-6 and Low-Reverse Piston Function Inspection
Table 5: | Input Speed Sensor Installation

### Fluid Seal Ring Installation

Callout | Component Name
--- | ---
1 | 3-5 Reverse and 4-5-6 Clutch Fluid Seal Ring

#### Procedure

1. Place J 46620-3 which is part of J-46620 seal installer over the case cover hub and adjust it so that only the bottom seal ring is exposed.
2. Place a NEW fluid seal ring onto J 46620-3 which is part of J-46620 seal installer .
3. Use J 46620-2 which is part of J-46620 seal installer to push the fluid seal ring down over J 46620-3 which is part of J-46620 seal installer into the hub ring groove.
4. Repeat the above steps to install all 4 seal rings, adjusting J 46620-3 which is part of J-46620 seal installer to the appropriate ring groove.

#### Special Tools

J-46620 Seal Installer

For equivalent regional tools, refer to Special Tools.

2 | Small Chamfer Up Caution: Do not force J 46620-1 down over the seals as this will roll and damage the seals. The large chamfer is designed to fit over the over stretched seal. Use a hand to help shrink the seal if J 46620-1 is difficult to install over the seal rings.

#### Procedure

Install J 46620-1 which is part of J-46620 seal installer with the large chamfer end down over the fluid seal rings and leave J 46620-1 which is part of J-46620 seal installer on the seals for at least 60 seconds.

3 | Large Chamfer Up

#### Procedure

1. Install J 46620-1 which is part of J-46620 seal installer with the small chamfer end facing down for at least 60 seconds. This will properly size the bottom seal ring.
2. Leaving J 46620-1 which is part of J-46620 seal installer on the fluid seal rings for an extended period of time could cause a fluid leak on the initial clutch piston circuit until the seal rings warm up and expand to the proper dimension.

### 2-6 Clutch Piston Installation

Callout | Component Name
--- | ---
1 | 2-6 Clutch Piston

#### Procedure

J-46621 seal protector prevents the piston seal lip from damage over the retaining ring groove during installation. Apply a thin coat of ATF to the O.D. of J-46621 seal protector to ease the installation of the piston.

#### Special Tools

J-46621 Seal Protector

For equivalent regional tools, refer to Special Tools.

2 | 2-6 Clutch Spring Assembly
3 | 2-6 Clutch Spring Assembly

#### Procedure

1. Install the retaining ring with the opening positioned to the top of the case cover.
2. Place the retainer ring inside J-46632 spring compressor prior to placing J-46632 spring compressor onto the spring.

#### Special Tools

J-46632 Spring Compressor

For equivalent regional tools, refer to Special Tools.

### Low and Reverse Clutch Piston Installation

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Piston Assembly

#### Procedure

1. Install the L/R piston with the air bleed positioned at the alignment feature on the cover, using J-46628-1 seal protector . This will orient the piston fingers with the openings in the case.
2. J-46628-1 seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of J-46628-1 seal protector to ease the installation of the piston.

#### Special Tools

J-46628-1 Piston Seal Protector

For equivalent regional tools, refer to Special Tools.

2 | Low and Reverse Clutch Spring
3 | Low and Reverse Clutch Spring Retaining Ring Tip Do not align the retainer opening with other retaining ring openings.

#### Special Tools

J-46628-2 Spring Compressor

For equivalent regional tools, refer to Special Tools.

### 2-6 and Low-Reverse Piston Function Inspection

Callout | Component Name
--- | ---
1 | Case Cover Assembly Tip The fluid seal rings should be in place and not damaged.
2 | 2-6 Clutch Feed Passage Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals.

#### Procedure

Apply shop air to the 2-6 clutch feed. Observe the 2-6 piston movement.

Tip
Minimal piston movement and excessive air leaking could indicate damage to the 2-6 piston seals or improper assembly.

3 | Low and Reverse Clutch Feed Passage Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals.

#### Procedure

Apply shop air to the Low and Reverse clutch feed. Observe the Low and Reverse piston movement.

Tip
Minimal piston movement and excessive air leaking could indicate damage to the Low and Reverse piston seals or improper assembly.

### Input Speed Sensor Installation

Callout | Component Name
--- | ---
1 | Input Speed Sensor Seal
2 | A/Trans Input Speed Sensor Assembly
3 | A/Trans Input Speed Sensor Bolt M6 x 25 Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Apply threadlocker GM P/N 12345382 (Canadian P/N 10953489) or equivalent to the input speed sensor bolt.

Tip
The seal is coated with a dry lubricant. If the coating is missing, lubricate the seal with automatic transmission fluid prior to installation.

Tighten
9 N·m (7 lb ft)