For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the body side trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the liftgate close actuator control module. Refer to Liftgate Actuator Replacement.

1 | Liftgate Close Actuator Bracket Bolt (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m (22 lb ft)
2 | Liftgate Close Actuator Bracket