For 1990-2009 cars

Note: Make any adjustments to camber before setting toe.

Note: Left side toe adjustment is shown, right side toe adjustment is similar.

1. Loosen the adjuster nut (1).
2. Using a wrench to rotate the adjuster bolt (2), adjust the cam (3) to specifications.

Caution: Refer to Fastener Caution in the Preface section.

Note: Ensure that the toe settings have not changed after torquing the adjuster nut to specifications. Readjust if necessary.

3. Using a wrench to hold the adjuster bolt (2), tighten the adjuster nut (1).

Tighten
Tighten the nut to 140 N·m (103 lb ft).

4. Check the toe alignment and adjust if required. Refer to Rear Toe Adjustment.
5. Test drive the vehicle.