For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Preliminary Procedure

Disconnect the hood strut rod. Refer to Hood Strut Replacement.

1 | Hood Hinge Pivot Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Hood Strut Tip

• | Disconnect windshield washer hose.

• | Transfer any parts as needed.

3 | Hood