For 1990-2009 cars

### Removal Procedure

1. Remove the engine mount strut and bracket. Refer to Engine Mount Strut Replacement - Right Side and Engine Mount Strut Bracket Replacement - Right Side.
2. Disconnect the engine wiring harness electrical connector (1) from the bank 1 intake camshaft position (CMP) sensor (2).
3. Remove the CMP sensor bolt and sensor (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the CMP sensor (2) and bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

2. Connect the engine wiring harness electrical connector (1) to the bank 1 intake CMP sensor (2).
3. Install the engine mount strut and bracket. Refer to Engine Mount Strut Replacement - Right Side and Engine Mount Strut Bracket Replacement - Right Side.