For 1990-2009 cars

### Removal Procedure

1. Remove the engine front cover. Refer to Engine Front Cover Replacement.
2. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement.

Important: If the entire camshaft timing system is not in stage 2 ( Camshaft Timing Drive Chain Alignment Diagram ), mark the timing chain and sprockets in order to ensure proper reassembly.

3. Remove the primary camshaft drive chain tensioner. Refer to Primary Camshaft Intermediate Drive Chain Tensioner Removal.

### Installation Procedure

1. Install the primary camshaft drive chain tensioner. Refer to Primary Camshaft Intermediate Drive Chain Tensioner Installation.
2. Install the spark plugs. Refer to Spark Plug Replacement.
3. Install the engine front cover. Refer to Engine Front Cover Replacement.